!
! No configuration change since last restart
!
version 12.4
service timestamps debug datetime msec localtime show-timezone year
service timestamps log datetime msec localtime show-timezone year
service password-encryption
!
hostname IPv6-relay
!
boot-start-marker
boot-end-marker
!
logging buffered 16384 debugging
no logging console
enable secret 5 $1$c2kX$b9n3xuP1IWqm2wtlmZXVP1
!
aaa new-model
!
aaa authentication login default local
aaa authentication enable default enable
!
aaa session-id common
clock timezone BDT 6
no network-clock-participate slot 1 
no network-clock-participate wic 0 
ip cef
!
no ip domain lookup
ip domain name workshop.net
ip auth-proxy max-nodata-conns 3
ip admission max-nodata-conns 3
!
ipv6 unicast-routing
ipv6 cef
!
username cisco secret 5 $1$YFYl$2EmmQ7nTh1.hl1tYZVRbX/
!
interface Loopback0
 ip address 192.88.99.1 255.255.255.255
!
interface Tunnel2002
 description 6to4 Tunnel
 no ip address
 no ip redirects
 ipv6 address 2002:C058:6301::/128
 tunnel source Loopback0
 tunnel mode ipv6ip 6to4
 tunnel path-mtu-discovery
!
interface FastEthernet0/0
 ip address 192.168.1.3 255.255.255.0
 duplex auto
 speed auto
!
interface Serial0/0
 no ip address
 shutdown
!
interface FastEthernet0/1
 no ip address
 shutdown
 duplex auto
 speed auto
!
interface Serial0/1
 no ip address
 shutdown
!
router bgp 49000
 no synchronization
 bgp log-neighbor-changes
 network 192.88.99.0
 network 192.168.1.0
 neighbor 192.168.1.254 remote-as 2
 no auto-summary
!
ip forward-protocol nd
ip route 0.0.0.0 0.0.0.0 192.168.1.254
ip route 10.0.0.0 255.0.0.0 Null0
ip route 127.0.0.0 255.0.0.0 Null0
ip route 169.254.0.0 255.255.0.0 Null0
ip route 172.16.0.0 255.240.0.0 Null0
ip route 192.0.2.0 255.255.255.0 Null0
ip route 192.88.99.0 255.255.255.0 Null0
ip route 192.168.0.0 255.255.0.0 Null0
!
no ip http server
no ip http secure-server
!
logging trap debugging
ipv6 route 2002::/16 Tunnel2002
!
control-plane
!
banner login ^C
IPv6 Workshop Tunnel Relay Router ^C
!
line con 0
 transport preferred none
line aux 0
line vty 0 4
 transport preferred none
 transport input ssh
 transport output telnet ssh
!
scheduler allocate 20000 1000
ntp clock-period 17179874
ntp server 192.168.1.2
!
end
